**Description:**

Type: BROEN BALLOMAX

Art. No.: 63.601

Pressure: PN 40

Dimension: DN 015 to DN 050

**Configuration:**

Fully welded branching valve with full bore and female/weld connection. Especially designed for use in central heating, heating, cooling and industry plants. Branching valve with plug for welding before insulation, ball with slot for indication of direction.

Valves are approved according to the directive for pressure equipment PED 2014/68/EU, Module H. and manufactured in accordance with ISO9001:2008 and ISO 14001.

**Technical data:**

Connection: Female/Weld

Temperature: Continuously 140 °C

Media: Neutral water, which do not corrode steel

House: Steel P235GH (St. 37)

O-ring: EPDM   
Ball: Stainless steel AISI 304L   
Seat packing: Reinforced PTFE 20% C, seat ring guide in RS steel and spring release

Operation: Unbraco key.

Surface: Enviromentally friendly corrosion resistant paint.

**Labeling:**

Maker, Dimension, Pressure, Temperature range, Production month and year.

CE marked