**Description:**

Type: BROEN BALLOMAX

Art. No.: 68.602

Pressure: PN 25

Dimension: DN 015 to DN 040

**Configuration:**

Fully welded hot tapping valve with full bore and weld/weld connection. Especially designed for use in district heating, heating, cooling and industry plants. Hot tapping valve with plug for welding before insulation, ball with slot for indication of direction of ball. Only original hot tapping valve tools are to be used according to makers instructions. The valves are approved according to the directive for pressure equipment PED 2014/68/EU, Module H. and manufactured according to ISO9001:2008 and ISO14001.

**Technical data:**

Connection: Weld/Weld

Temperature: Continuously 140 °C

Media: Treated water to avoid corrosion/lime formation

House: Steel P235GH (St. 37)

O-ring: EPDM   
Ball: Stainless steel AISI 304L   
Seatpacking: Reinforced PTFE 20% C

Operation: Unbraco key and/or wrench key.

Surface: Enviromentally friendly corrosion resistant paint.

**Labeling:**

Maker, Dimension, Pressure, Temperature range, Productions month and year.

CE marked

**Accesory:**

Hot tapping tools for respective dimensions.