**Description:**

Type: BROEN BALLOMAX

Art. No.: 55.100

Pressure: PN 40

Dimension: DN10 to DN50

**Configuration:**

Fully welded ball valve with reduced bore and female/female connection. Especially designed for use in central heating, heating, cooling and industrial plants. Stem and stop made in stainless steel with double sealings in stuffing box with Graphite rings. The valves are manufactured according to ISO9001:2008 and ISO14001.

**Technical data:**

Connection: Female/female

Temperature: Continuously 250 °C

Media: Treated water to avoid corrosion/lime formation, suitable for steam

House: Steel P235GH (St. 37)

Rings: Graphite (Grafmet 950)

Ball: Stainless Steel AISI 304L

Seat packing: Reinforced PTFE 20%C

Operation: Handle

Surface: Environmentally corrosion resistant paint

**Labeling:**

Maker, Dimension, Pressure step, Temperature range, Production month and year.