**Description:**

Type: BROEN BALLOMAX

Art. No.: 69.302…

Pressure: PN 25

Dimension: DN 015 to DN 025

**Configuration:**

Main stop valves mounted on heavy steel bracket with possible adjustable mounting on wall and variable adjustment of the valves individual location.

Fully welded ball valve with reduced bore and weld/weld connection. Especially designed for use in central heating, straight single pipes. Stem and stop made in stainless steel with double sealings in stuffing box with exchangeable o-rings.

The valves are approved according to the directive for pressurized equipment PED 2014/68/EU, Module H. and manufactured according to ISO9001:2008 and ISO14001.

**Technical data:**

Connection: Weld / Weld

Temperature: Continuous 140 °C

Media: Treated water to avoid corrosion/lime formation

House: Steel P235GH (St. 37)

O-rings: EPDM and Viton

Ball: Stainless Steel AISI 304L

Seat packing: Reinforced PTFE 20%C

Operation: T-handle Red/Blue, reversible

Surface: Environmentally corrosion resistant paint

**Labeling:**

Maker, Dimension, Pressure step, Temperature range, Production month and year.

CE marked.

**Accessories:**

Yellow T-handle

DN020 & DN025 Insulation shells

Extra bracket for extension

Locking bracket