**Description:**

Type: BROEN BALLOMAX

Art. Nr.: 500566 to 500827

Dimension: From DN 080 up to DN 500

**Configuration:**

Manually operated worm gear with hexagon for slow opening and closing of steelballvalves. The gear is mounted on the valve by means of ISO flange and 4 belonging bolts. The worm has to be greased with temperature resistant grease up to 90°C. The gear is with adjustable end stops and is adjusted acc. To makers regulations.

**Technical data:**

Temperature: Up to 90°C (At higher temperature special grease is to be used)

Mounting: ISO-flange and fitted actual stem dimension.

Material: Casted steel gear box, stainless gear rod and hexagon.

Surface: Environmentally friendly corrosion resistant paint.

**Labelling:**

Maker, dimension, temperature range, production month and year.

**Accesories:**

Endstop contact/switch with signal outtake.